A new negative refractive index (NRI) metamaterial unit cell is presented in this study. The negative refractive index property is being displayed by the unit cell of metamaterial in the four distinct microwave frequency bands. Finite integration technique was adopted to evaluate the property of the material. More than 1 GHz bandwidth region was found exhibiting NRI property for the material in the microwave spectra.
